|  |  |
| --- | --- |
| **ESP32** | **SIM800L** |
| GND | GND |
| D2 | Tx |
| D4 | Rx |
| Vin (in D13 row) | Vcc |

NOTE: -

SoftwareSerial serialGsm(2, 4); // RX, TX pins for communicating with modem

Rx of SIM800L will be Tx for ESP32 and vise verse